6800 SERIES PAGE

H1 **Feature Options**

H2 **Certifications**

UL Standard 437 compliant\*

EN 1300 Class B compliant\*\*

\* *Model 6870*

*\*\* Model 6880*

H2 **Operation**

Opposing lever design.

Advanced pick resistance.

Double-bitted lock with opposing brass levers.

Key-retaining design.

Key-changeable without disassembling the lock.

Standard mounting footprint.

Keyhole collocated with spindle hole.

Keys available in 4 different lengths.

H2 **Warranty**

One-year limited warranty from date of shipment.

H1 **Product options**

H2 **Model 6870**

Duplicate and replacement keys available.

Suitable for North American applications.

H2 **Model 6880**

Limited key codes.

Suitable for European applications.